How to build a MaxFrame for REAL/32 disk set using DISKCOPY
===========================================================

Diskette image files are in 1.44MB format for 3.50" Floppy Disks.

You will need three 3.5" 1.44MB diskettes.

For each diskette image file run the DISKCOPY command, specifying 
the filename followed by the destination drive as follows:

	DISKCOPY MAX774_1.350 A:
	DISKCOPY MAX774_2.350 A:
	DISKCOPY MAX774_3.350 A:


Label the first diskette "Disk 1". Label subsequent diskettes
"Disk 2" and "Disk 3"

You need to have ims REAL/32 installed on your system, and you
can obtain evaluation copies at www.imsltd.com.

[Last Updated 30 Jan 2001]
